# POST LAB

//RA2111004010177

module FS(diff, borr, a, b, c); output diff; output borr; input a; input b; input c;

assign diff = a^b^c; assign borr = c&(a^b)|(~a&b); endmodule

## FULL SUBTRACTOR OUTPUT WAVEFORM USING XILINX

